**PPD Substantial Completion Checklist**

CM/GC shall be responsible for following inspections and reviews and obtaining PPD approval for the building sub-system for substantial completion.

|  |  |  |
| --- | --- | --- |
| **11** | Building Plumbing/fixtures | Approved for Substantial Completion:(Required for Substantial Completion Approval by PPD Office.) |
|  | Inspection/Review Item | **Notice Required** | **Remarks** |
| 1 | Initial pressure testing of the system | 24 hours | Must be witnessed and signed off by PPD Operations Engineering. |
| 2 | Piping, valves, drains, leaks | 60% Completion | Inspections must be conducted before piping is covered |
| 3 | Water closet, flush system Water Closet fixturesWater fountains | One week prior to SCI |  |
| 4 | Field/Change orders | At all phases | See general notes. |