**PPD Construction Administration Checklist**

CM/GC shall be responsible for following inspections, reviews and obtaining PPD approval for the building subsystem for substantial completion.

|  |  |  |
| --- | --- | --- |
| **9** | Building Potable Water Systems | Approved for Substantial Completion:(Required for Substantial Completion Approval by PPD Office.) |
|  | **Inspection/Review Item** | **Notice Required** | **Remarks** |
|  1 | Piping / valve installations. Verify metering.Check Drain System | 60% Completion |  |
|  2 | Flushing & SterilizingWater Sampling | 24 hours | Must be witnessed & signed off by PPD Operations Engineering.Must be witnessed by and sampling results returned to PPD Operations Engineering. |
|  3 | Valve Charts | One week prior to SCI  | Must be in a location within the building, framed or laminated. |
|  4 | Field/Change order | At all phases | See general notes. |