**PPD Construction Administration Checklist**

CM/GC shall be responsible for following inspections and reviews and obtaining PPD approval for the building sub-system for substantial completion.

|  |  |  |
| --- | --- | --- |
| **20** | **Landscaping and Solid Waste Management** | Approved for Substantial Completion:(Required for Substantial Completion Approval by PPD) |
|  | Inspection/Review Item | **Notice Required** | **Remarks** |
|  | **Landscaping** |  |  |
|  1 | Tree Barricades | Prior to site mobilization | Contractor erects barricades as shown on the Tree Barricade Plan, then call for inspection. |
|  2 | Digging within BarricadesTrimming overhanging limbs | Prior to the start of work | Contactor calls PPD Grounds before moving barricades or entering the barricaded area to dig.Limbs that are blocking access to work areas may be trimmed with PPD consultation. |
|  3 | Preserved/Saved landscaping | 48 hours prior to new install. | Final inspection of preserved vegetation before installation of new landscaping is required. |
|  4 | New Landscaping | Immediately after install. | Contractor provides evidence of correct plant material location, size, species, quality and quantity. |
|  | **Solid Waste Management** |  |  |
|  5 | Waste management mockup | 72 hours prior to hardscape installation | Stake out a mockup of driveway/access way and call for test run with PPD’s waste management truck. |
|  6 | Waste management infrastructure | Within 72 hours after hardscape installation has dried | Verification of final construction adequacy, accessibility to servicing equipment at the refuse/recycling facilities. |