**PPD Construction Administration Checklist**

CM/GC shall be responsible for following inspections and reviews and obtaining PPD approval for the building sub-system for substantial completion.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **20** | | **Landscaping and Solid Waste Management** | | Approved for Substantial Completion:  (Required for Substantial Completion Approval by PPD) | |
|  | Inspection/Review Item | **Notice Required** | **Remarks** |
|  | **Landscaping** |  |  |
| 1 | Tree Barricades | Prior to site mobilization | Contractor erects barricades as shown on the Tree Barricade Plan, then call for inspection. |
| 2 | Digging within Barricades  Trimming overhanging limbs | Prior to the start of work | Contactor calls PPD Grounds before moving barricades or entering the barricaded area to dig.  Limbs that are blocking access to work areas may be trimmed with PPD consultation. |
| 3 | Preserved/Saved landscaping | 48 hours prior to new install. | Final inspection of preserved vegetation before installation of new landscaping is required. |
| 4 | New Landscaping | Immediately after install. | Contractor provides evidence of correct plant material location, size, species, quality and quantity. |
|  | **Solid Waste Management** |  |  |
| 5 | Waste management mockup | 72 hours prior to hardscape installation | Stake out a mockup of driveway/access way and call for test run with PPD’s waste management truck. |
| 6 | Waste management infrastructure | Within 72 hours after hardscape installation has dried | Verification of final construction adequacy, accessibility to servicing equipment at the refuse/recycling facilities. |