**PPD Construction Administration Checklist**

CM/GC shall be responsible for following inspections and reviews and obtaining PPD approval for the building sub-system for substantial completion.

|  |  |  |  |
| --- | --- | --- | --- |
| **2** | Demolition | | Approved for Substantial Completion:  (Required for Substantial Completion Approval by PPD Office.) |
|  | Inspection/Review Item | **Notice Required** | **Remarks** | |
| 1 | All Demolition | 24 hours | All drop ceiling grid and hangers (wire or otherwise) removed.  All ductwork and hangers removed.  Remove all items being disconnected.  Leave nothing abandoned in place inside the buildings unless preapproved. | |